.. _wave:

WAVE: Heatmap Generation 
------------------------

WAVE (WiFi Area Visual Evaluator) turns measurement logs from STAT into heatmaps.

    1. Open the SWiSS application on the laptop and select WAVE (WiFi Area Visual Evaluator):
    
    .. image:: images/swiss_wave.png

    2. Select the JSON configuration file within the STAT log directory to generate the heatmaps.

    .. image:: images/swiss_wave_load_config.png

    3. The generated heatmaps can be exported to image files by accessing the menu item (**File->Export Heatmap As Images**) from the top menu bar: 

    .. image:: images/swiss_wave_heatmap.png
