# SWiSS User Guide

Author: Dareun Geum

Version: v1.0

SWiSS (Spatial WiFi Site Survey) toolkit is a collection of tools designed to facilitate indoor and outdoor WiFi HaLow coverage testing and analysis. This tutorial will cover the basic usage of the toolkit and illustrate a typical workflow.

The SWiSS toolkit consists of five components:

> 1. STAT: Spatial Test Automation Tool

>      - (STA-side) Automated measurement logging tool

> 2. WAVE: WiFi Area Visual Evaluator

>      - Heatmap generation tool

> 3. Instructions

>      - Web-based documentation on SWiSS usage

> 4. SPOT: Spatial Position Organizing Tool

>      - Spatial coordinate marking tool

> 5. SCAN: Station Control & Activity Nexus

>      - (AP-side) STA activity monitoring tool

## Requirements

> - The tool requires Java Runtime Environment (JRE8). Download and install the OS-compatible version of JRE8 for the PC.

> - The SWiSS AP/STA servers need to be running on the EVK. For enabling SWiSS on older EVKs, refer to the NRC7394 EVK User Guide web documentation for more information.

Main Tool Usage:

- STAT: Introduction
- STAT: Data Collection (with GPS)
- STAT: Data Collection (Without GPS)
- WAVE: Heatmap Generation

Supplementary Tool Usage:

- SPOT: Manual Coordinate Marking
- SCAN: AP-Side Monitoring